From e5bf80f2fb4af9a2627541cb8bc8686e8a9e8404 Mon Sep 17 00:00:00 2001
From: Jason Kridner <jdk@ti.com>
Date: Tue, 6 Sep 2011 18:56:11 -0400
Subject: [PATCH 16/21] beagleboard: config: enable gpio command

Now that we are using the generic GPIO framework, enable the command.
---
 include/configs/omap3_beagle.h |    1 +
 1 files changed, 1 insertions(+), 0 deletions(-)

diff --git a/include/configs/omap3_beagle.h b/include/configs/omap3_beagle.h
index 569d747..337ca29 100644
--- a/include/configs/omap3_beagle.h
+++ b/include/configs/omap3_beagle.h
@@ -164,6 +164,7 @@
 #define CONFIG_CMD_PING
 #define CONFIG_CMD_DHCP
 #define CONFIG_CMD_SETEXPR	/* Evaluate expressions		*/
+#define CONFIG_CMD_GPIO
 
 #undef CONFIG_CMD_FLASH		/* flinfo, erase, protect	*/
 #undef CONFIG_CMD_FPGA		/* FPGA configuration Support	*/
-- 
1.7.2.5

