From 1f6651f5448df6b40e8feafccceed942f192a430 Mon Sep 17 00:00:00 2001
From: Daniel Schwierzeck <daniel.schwierzeck@googlemail.com>
Date: Thu, 23 Feb 2012 17:59:49 +0100
Subject: [PATCH 09/60] mtd: mips: lantiq: reintroduce support for cmdline
 partitions

commit bf011f2ed53d587fdd8148c173c4f09ed77bdf1a upstream.

Since commit ca97dec2ab5c87e9fbdf7e882e1820004a3966fa the
command line parsing of MTD partitions does not work anymore.

Signed-off-by: Daniel Schwierzeck <daniel.schwierzeck@googlemail.com>
Signed-off-by: John Crispin <blogic@openwrt.org>
Signed-off-by: Artem Bityutskiy <artem.bityutskiy@linux.intel.com>
Acked-by: John Crispin <blogic@openwrt.org>
Signed-off-by: David Woodhouse <David.Woodhouse@intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/mtd/maps/lantiq-flash.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/drivers/mtd/maps/lantiq-flash.c b/drivers/mtd/maps/lantiq-flash.c
index 4f10e27..764d468 100644
--- a/drivers/mtd/maps/lantiq-flash.c
+++ b/drivers/mtd/maps/lantiq-flash.c
@@ -45,6 +45,7 @@ struct ltq_mtd {
 };
 
 static char ltq_map_name[] = "ltq_nor";
+static const char *ltq_probe_types[] __devinitconst = { "cmdlinepart", NULL };
 
 static map_word
 ltq_read16(struct map_info *map, unsigned long adr)
@@ -168,7 +169,7 @@ ltq_mtd_probe(struct platform_device *pdev)
 	cfi->addr_unlock1 ^= 1;
 	cfi->addr_unlock2 ^= 1;
 
-	err = mtd_device_parse_register(ltq_mtd->mtd, NULL, 0,
+	err = mtd_device_parse_register(ltq_mtd->mtd, ltq_probe_types, 0,
 			ltq_mtd_data->parts, ltq_mtd_data->nr_parts);
 	if (err) {
 		dev_err(&pdev->dev, "failed to add partitions\n");
-- 
1.7.9.5

