From c194377152df812bcb29fff8f217ffbde59089be Mon Sep 17 00:00:00 2001
From: Aaro Koskinen <aaro.koskinen@nokia.com>
Date: Thu, 24 Mar 2011 18:35:35 +0200
Subject: [PATCH 07/12] OMAP3+: smartreflex: delete debugfs entries on probe error

Delete created debugfs entries if probe fails.

Signed-off-by: Aaro Koskinen <aaro.koskinen@nokia.com>
Signed-off-by: Kevin Hilman <khilman@ti.com>
Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/smartreflex.c |    6 ++++--
 1 files changed, 4 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/smartreflex.c b/arch/arm/mach-omap2/smartreflex.c
index f0a488a..fb7dc52 100644
--- a/arch/arm/mach-omap2/smartreflex.c
+++ b/arch/arm/mach-omap2/smartreflex.c
@@ -929,7 +929,7 @@ static int __init omap_sr_probe(struct platform_device *pdev)
 		dev_err(&pdev->dev, "%s: Unable to create debugfs directory"
 			"for n-values\n", __func__);
 		ret = PTR_ERR(nvalue_dir);
-		goto err_iounmap;
+		goto err_debugfs;
 	}
 
 	omap_voltage_get_volttable(sr_info->voltdm, &volt_data);
@@ -939,7 +939,7 @@ static int __init omap_sr_probe(struct platform_device *pdev)
 			"entries for n-values\n",
 			__func__, sr_info->voltdm->name);
 		ret = -ENODATA;
-		goto err_iounmap;
+		goto err_debugfs;
 	}
 
 	for (i = 0; i < sr_info->nvalue_count; i++) {
@@ -953,6 +953,8 @@ static int __init omap_sr_probe(struct platform_device *pdev)
 
 	return ret;
 
+err_debugfs:
+	debugfs_remove_recursive(sr_info->dbg_dir);
 err_iounmap:
 	list_del(&sr_info->node);
 	iounmap(sr_info->base);
-- 
1.6.6.1

