From 132469e10e712ff4b386fb78a4c78343f151ebc4 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Sun, 18 Jul 2010 11:25:12 +0200
Subject: [PATCH 65/75] rtl8192su: remove bogus Kconfig depend on PCI and add another product ID

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 drivers/staging/rtl8192su/Kconfig       |    2 +-
 drivers/staging/rtl8192su/r8192U_core.c |    1 +
 2 files changed, 2 insertions(+), 1 deletions(-)

diff --git a/drivers/staging/rtl8192su/Kconfig b/drivers/staging/rtl8192su/Kconfig
index 123fa6d..9888927 100644
--- a/drivers/staging/rtl8192su/Kconfig
+++ b/drivers/staging/rtl8192su/Kconfig
@@ -1,6 +1,6 @@
 config RTL8192SU
 	tristate "RealTek RTL8192SU Wireless LAN NIC driver"
-	depends on PCI && WLAN && USB
+	depends on WLAN && USB
 	depends on WIRELESS_EXT
 	default N
 	---help---
diff --git a/drivers/staging/rtl8192su/r8192U_core.c b/drivers/staging/rtl8192su/r8192U_core.c
index 66274d7..48e4c29 100644
--- a/drivers/staging/rtl8192su/r8192U_core.c
+++ b/drivers/staging/rtl8192su/r8192U_core.c
@@ -112,6 +112,7 @@ u32 rt_global_debug_component = \
 
 static struct usb_device_id rtl8192_usb_id_tbl[] = {
 	/* Realtek */
+	{USB_DEVICE(0x0bda, 0x8171)},
 	{USB_DEVICE(0x0bda, 0x8192)},
 	{USB_DEVICE(0x0bda, 0x8709)},
 	/* Corega */
-- 
1.6.6.1

