From 6bdb8e890f8e5d11be3c4953d7d10f4a5f160cd4 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Thu, 21 Jul 2011 12:59:20 +0200
Subject: [PATCH 2/3] HACK: OMAP3: beagle: switch to GPTIMER1

Breaks with B3 and older due to clock noise

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index f26a9a8..a04f5a0 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -832,5 +832,5 @@ MACHINE_START(OMAP3_BEAGLE, "OMAP3 Beagle Board")
 	.init_early	= omap3_beagle_init_early,
 	.init_irq	= omap3_beagle_init_irq,
 	.init_machine	= omap3_beagle_init,
-	.timer		= &omap3_secure_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
-- 
1.6.6.1

