Getting a probe response after sending a probe request to a specific SSID
doesnt mean we're trying to associate with this SSID.
wpa_supplicant should be the only one deciding when to join an SSID, not the
kernel.

Signed-off-by: Samuel Ortiz <sameo@linux.intel.com>
---
 drivers/staging/rtl8192e/ieee80211/ieee80211_rx.c |    4 ----
 1 file changed, 4 deletions(-)

Index: b/drivers/staging/rtl8192e/ieee80211/ieee80211_rx.c
===================================================================
--- a/drivers/staging/rtl8192e/ieee80211/ieee80211_rx.c	2010-01-15 16:56:47.000000000 +0100
+++ b/drivers/staging/rtl8192e/ieee80211/ieee80211_rx.c	2010-01-15 16:57:03.000000000 +0100
@@ -2716,8 +2716,6 @@ static inline void ieee80211_process_pro
 #endif
 		memcpy(target, &network, sizeof(*target));
 		list_add_tail(&target->list, &ieee->network_list);
-		if(ieee->softmac_features & IEEE_SOFTMAC_ASSOCIATE)
-			ieee80211_softmac_new_net(ieee,&network);
 	} else {
 		IEEE80211_DEBUG_SCAN("Updating '%s' (" MAC_FMT ") via %s.\n",
 				     escape_essid(target->ssid,
@@ -2744,8 +2742,6 @@ static inline void ieee80211_process_pro
 		//YJ,add,080819,for hidden ap,end
 
 		update_network(target, &network);
-		if(renew && (ieee->softmac_features & IEEE_SOFTMAC_ASSOCIATE))
-			ieee80211_softmac_new_net(ieee,&network);
 	}
 
 	spin_unlock_irqrestore(&ieee->lock, flags);

-- 
Intel Open Source Technology Centre
http://oss.intel.com/
_______________________________________________
Moblin-kernel mailing list
Moblin-kernel@linux.intel.com
http://linux.intel.com/mailman/listinfo/moblin-kernel

