From d134dafc2f11e0d247420a0ba360bcdef77b4093 Mon Sep 17 00:00:00 2001
From: Andre McCurdy <armccurdy@gmail.com>
Date: Tue, 19 Jan 2016 16:00:00 -0800
Subject: [PATCH] use appropriate -march/-mcpu/-mfpu for ARM test apps

Ensure that test apps in none/tests/arm are compiled with appropriate
-march/-mcpu/-mfpu flags to support the instructions being tested.
The aim is to build all tests, even ones which may not run correctly
on all target CPUs.

For tests requiring armv7ve instructions, ensure that we set both
-march=armv7ve and -mcpu=cortex-a15 (since some TUNE_CCARGS may set
-march=armv7-a and adding -mcpu=cortex-a15 alone is not enough to
over-ride that).

See similar cases in none/tests/arm/Makefile.am

Upstream-Status: Pending

Signed-off-by: Andre McCurdy <armccurdy@gmail.com>
---
 none/tests/arm/Makefile.am | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

diff --git a/none/tests/arm/Makefile.am b/none/tests/arm/Makefile.am
index 4507a20..825290f 100644
--- a/none/tests/arm/Makefile.am
+++ b/none/tests/arm/Makefile.am
@@ -62,8 +62,10 @@ neon64_CFLAGS     = $(AM_CFLAGS) -g -O0 -mcpu=cortex-a8 \
 			-mfpu=neon \
 			-mthumb
 
-intdiv_CFLAGS	  = $(AM_CFLAGS) -g -mcpu=cortex-a15 -mthumb
+intdiv_CFLAGS	  = $(AM_CFLAGS) -g -march=armv7ve -mcpu=cortex-a15 -mthumb
 ldrt_CFLAGS	  = $(AM_CFLAGS) -g -mcpu=cortex-a8 -mthumb
 ldrt_arm_CFLAGS	  = $(AM_CFLAGS) -g -mcpu=cortex-a8 -marm
 
-vfpv4_fma_CFLAGS  = $(AM_CFLAGS) -g -O0 -mcpu=cortex-a15 -mfpu=vfpv4 -marm
+vcvt_fixed_float_VFP_CFLAGS = $(AM_CFLAGS) -g -mcpu=cortex-a8 -mfpu=vfpv3
+
+vfpv4_fma_CFLAGS  = $(AM_CFLAGS) -g -O0 -march=armv7ve -mcpu=cortex-a15 -mfpu=vfpv4 -marm
-- 
1.9.1

