## rtl8188eus v5.7.6.1

# Realtek rtl8188eus &amp; rtl8188eu &amp; rtl8188etv WiFi driver

[![Monitor mode](https://img.shields.io/badge/monitor%20mode-supported-brightgreen.svg)](#)
[![Frame Injection](https://img.shields.io/badge/frame%20injection-supported-brightgreen.svg)](#)
[![MESH Mode](https://img.shields.io/badge/mesh%20mode-supported-brightgreen.svg)](#)
[![GitHub issues](https://img.shields.io/github/issues/aircrack-ng/rtl8188eus.svg)](https://github.com/aircrack-ng/rtl8188eus/issues)
[![GitHub forks](https://img.shields.io/github/forks/aircrack-ng/rtl8188eus.svg)](https://github.com/aircrack-ng/rtl8188eus/network)
[![GitHub stars](https://img.shields.io/github/stars/aircrack-ng/rtl8188eus.svg)](https://github.com/aircrack-ng/rtl8188eus/stargazers)
[![GitHub license](https://img.shields.io/github/license/aircrack-ng/rtl8812au.svg)](https://github.com/aircrack-ng/rtl8188eus/blob/master/LICENSE)<br>
[![Android](https://img.shields.io/badge/android%20(8)-supported-brightgreen.svg)](#)
[![aircrack-ng](https://img.shields.io/badge/aircrack--ng-supported-blue.svg)](#)


# Supports
* Android 9
* WPA3-SAE
* P2P Mode
* WiFi Direct
* MESH Support
* Monitor mode
* Frame injection
* Supported up to kernel v5.10+
... And a bunch of various wifi chipsets

# Howto download/build/install
```sh
1. Clone the repo with "git clone https://github.com/aircrack-ng/rtl8188eus -b v5.7.6.1"
2. Enter the folder with "cd rtl8188eus"
2. Then run "make && make install"
3. And reboot in order to blacklist the module and load this module instead.
```

# MONITOR MODE howto
Use these steps to enter monitor mode.
```sh
$ airmon-ng check-kill
$ ip link set <interface> down
$ iw dev <interface> set type monitor
```
To set txpower to a higher level.
```sh
$ iw <interface> set txpower fixed 3000
```

Frame injection test may be performed with
```sh
$ aireplay -9 <interface>
```

# NetworkManager configuration
Add these lines below to "NetworkManager.conf" and ADD YOUR ADAPTER MAC below [keyfile]
This will make the Network-Manager ignore the device, and therefor don't cause problems.
```sh
[device]
wifi.scan-rand-mac-address=no

[ifupdown]
managed=false

[connection]
wifi.powersave=0

[main]
plugins=keyfile

[keyfile]
unmanaged-devices=mac:A7:A7:A7:A7:A7
```

